**Assembly instruction of 49cc mini atv**

1, assembly handle bar on (4 bolts), line up cables/wirings

2, set up rear shock(one bolt/nut)

3, set up front wheel/axle/tie rod.

4, adjust tie rods to make front wheels straightly. Then tight nuts on rods.

5, connect fuel pipe to carby.

6. front plastic fairing (3 bolts,just screw the top bolt in and not need nut, but the bottom 2 bolts need nuts )

7,fix 4 mudguards to brackets

8. chain cover.

9, check all bolts/nuts

10. mix fuel with oil. 25:1(1L unlead adds 40ml 2 stroke oil), add petrol into the tank

12, push choke level up, then pull start, choke level down.

13, kids must wear helmets/enclosed shoes/long sleeves/long pants before riding on it. Tie up long hair.

Thanks